**Specifications sheet**

**Material**  
» Aluminium Al Mg Si 0,5  
  
**Finishing**  
» Natural anodised: 20 to 22 micron  
» Dark bronze anodised: 20 to 22 micron  
» Powder-coated in any RAL-colour: pre-assembled product is conversed to ensure a solid adherence (Brugal) and powder-coated in order to guarantee a thorough powder-layer at all corner joints and cutting sections: 60 to 70 micron.  
  
**Description**  
» The perforated ventilation openings in the vertical frame profiles have a fixed width of 18 mm and the pitch is 22 mm.  
» Special heights can be manufactured upon request: these registers are made up from sections 67 mm, 100 mm, 130 mm or 150 mm.  
» Height: always 150, 200 or 300 mm.  
» Width: all sizes  
» Operation: with sliding knob. Registers longer than 500 mm are supplied with turning knob.  
» An insect screen in stainless stell 304 (18/8) is fitted as standard.  
» Controllable  
  
**Fixing**  
» Screws and plugs are supplied as standard.