**Specifications sheet**

**Material**
» Aluminium Al Mg Si 0,5

**Finishing**
» Natural anodised: 20 to 22 micron
» Dark bronze anodised: 20 to 22 micron
» Powder-coated in any RAL-colour: pre-assembled product is conversed to ensure a solid adherence (Brugal) and powder-coated in order to guarantee a thorough powder-layer at all corner joints and cutting sections: 60 to 70 micron.

**Description**
» The perforated ventilation openings in the vertical frame profiles have a fixed width of 18 mm and the pitch is 22 mm.
» Special heights can be manufactured upon request: these registers are made up from sections 67 mm, 100 mm, 130 mm or 150 mm.
» Height: always 150, 200 or 300 mm.
» Width: all sizes
» Operation: with sliding knob. Registers longer than 500 mm are supplied with turning knob.
» An insect screen in stainless stell 304 (18/8) is fitted as standard.
» Controllable

**Fixing**
» Screws and plugs are supplied as standard.