**Specifications sheet**

**Material**
» Aluminium Al Mg Si 0,5

**Finishing**
» Natural anodised: 20 to 22 micron
» Dark bronze anodised: 20 to 22 micron
» Powder-coated in any RAL-colour: pre-assembled product is conversed to ensure a solid adherence (Brugal) and powder-coated in order to guarantee a thorough powder-layer at all corner joints and cutting sections: 60 to 70 micron.

**Description**
» Window profiles with a total height of 21 mm and cut at mitre of 45° and assembled through compression and a clamping corner.
» The heights are always determined by the combination of the sliding ventilators type 100, 130 and 150 mm.
» Operation with sliding knob. Registers longer than 500 mm are supplied with turning knob.
» The sliding ventilator with vertical slots is equiped with an aluminiumand PVC slider which ensures a good wind tightness.

**Specification**
» Depth to fit: 28,5 mm
» Total thickness: 33,5 mm
» Flange size: 21 mm

**Fixing**
» Springclips no. 419 or dowels no. 418 can be supplied.