**Specifications sheet**

**Material**
» Units are assembled from extruded sections of stainless steel 316/L
» Bird mesh screen in stainless steel 304 - 6 X 6 mm

**Description**
» Frame profiles with a total height of 41,5 mm cut at mitre and assembled by
means of point welding.
» Minimum profile thickness: 1,5 mm
» The Z-shaped blades with a height of 50 mm are fixed in the frame by means of
point welding.
» The pitch of the blades is 34 mm.
» A bird mesh screen in stainless steel 304 (6 X 6 mm) is fitted as standard.

**Specification**
» Depth to fit: 43 mm
» Total thickness: 50 mm
» Flange size: 40 mm
» Visual free area: 70%

**Fixing**
» Fixing by means of dowels.