**Specifications sheet**

**Material**   
» Units are assembled from extruded sections of stainless steel 316/L   
» Bird mesh screen in stainless steel 304 - 6 X 6 mm   
  
**Description**   
» Frame profiles with a total height of 41,5 mm cut at mitre and assembled by   
means of point welding.   
» Minimum profile thickness: 1,5 mm   
» The Z-shaped blades with a height of 50 mm are fixed in the frame by means of   
point welding.   
» The pitch of the blades is 34 mm.   
» A bird mesh screen in stainless steel 304 (6 X 6 mm) is fitted as standard.   
  
**Specification**   
» Depth to fit: 43 mm   
» Total thickness: 50 mm   
» Flange size: 40 mm   
» Visual free area: 70%   
  
**Fixing**   
» Fixing by means of dowels.